
A close-up of a computer chip

AI-generated content may be incorrect.

**ADSBee 1090**

Open Source Embedded ADS-B Receiver



Features

* 1090MHz Mode S and ADS-B packet decoding.
* Adjustable receive gain and trigger levels for customized tuning in diverse RF environments.
* Tunable sub-GHz transceiver for UAT / additional protocols.
* Multiple output formats over UART or USB: Raw Frames / ADSBee CSV / MAVLINK1 / MAVLINK2 / Mode S Beast / GDL90
* GNSS module input (UART + PPS) for MLAT or Remote ID applications.
* 2.4GHz 802.11 module for connecting directly to ADS-B databases via WiFi or broadcasting Remote ID beacon frames in UAS applications.
* Integrated M2.5 mounting holes.
* Optional PoE pant for power + data over Ethernet.
* Firmware updates over USB, Serial, WiFi, Ethernet.

Applications

* Aircraft detection for robotics and embedded projects.
* Electronic Flight Bag ADS-B receiver.
* Standalone feeder device for online ADS-B databases. No external compute required, just add power and WiFi!

Quick Specs

|  |  |
| --- | --- |
| Supply Voltage | 5V (via USB or 5V pin) |
| Supply Current | 120mA (WiFi disabled)  ~400mA (WiFi enabled) |
| Minimum RF Input Power Level | -70dBm |
| Simultaneous Aircraft Tracks Supported | ≤400 |
| Connectors | 1090MHz RF In: U.FL / MHF1  Sub-GHz RF In/Out: U.FL / MHF1  802.11 RF Out: W.FL / MHF3  Power / Data: USB C  GPIO / UART: 0.1” Pin Headers |

Open Source Hardware + Software

Github Repository: <https://github.com/coolnamesalltaken/adsbee>

All hardware schematics and source code files required to build ADSBee 1090 are available under a GNU GPL v3 license. This means that they can be freely incorporated into other open-source projects that utilize a compatible license. The hope is that by opening the design to contributions and feedback from a community of users, the functionality of the ADSBee 1090 will be enhanced over time.

Note that the GPL v3 license applies to design and source code files, and not devices. ADSBee 1090 units purchased from Pants for Birds may be used in commercial applications without any licensing restrictions.

For commercial licensing requests of ADSBee hardware or software design files, please contact <john@pantsforbirds.com>.

Contents

[Features 1](#_Toc207586464)

[Applications 1](#_Toc207586465)

[Quick Specs 1](#_Toc207586466)

[Open Source Hardware + Software 1](#_Toc207586467)

[Revision History 5](#_Toc207586468)

[1 Background 6](#_Toc207586469)

[2 Communication Interfaces 6](#_Toc207586470)

[2.1 Console Interface 6](#_Toc207586471)

[2.2 COMMS\_UART Interface 6](#_Toc207586472)

[2.3 GNSS\_UART Interface 6](#_Toc207586473)

[3 AT Commands 7](#_Toc207586474)

[3.1 AT+BAUD\_RATE 7](#_Toc207586475)

[3.1.1 Set Baud Rate 7](#_Toc207586476)

[3.1.2 Query Baud Rate 7](#_Toc207586477)

[3.2 AT+BIAS\_TEE\_ENABLE 8](#_Toc207586478)

[3.2.1 Turn the Bias Tee On or Off 8](#_Toc207586479)

[3.2.2 Query the Status of the Bias Tee 8](#_Toc207586480)

[3.3 AT+DEVICE\_INFO 8](#_Toc207586481)

[3.4 AT+ESP32\_ENABLE 9](#_Toc207586482)

[3.4.1 Turn the ESP32 On or Off 9](#_Toc207586483)

[3.4.2 Query the Status of the ESP32 9](#_Toc207586484)

[3.5 AT+ESP32\_FLASH 9](#_Toc207586485)

[3.6 AT+ETHERNET 9](#_Toc207586486)

[3.6.1 Enable or Disable Ethernet 9](#_Toc207586487)

[3.6.2 Query Ethernet Setting 9](#_Toc207586488)

[3.7 AT+FEED 9](#_Toc207586489)

[3.7.1 Configure a Feed 9](#_Toc207586490)

[3.7.2 Query Configuration of All Feeds 11](#_Toc207586491)

[3.7.3 Query Configuration of a Single Feed 12](#_Toc207586492)

[3.8 AT+HELP 12](#_Toc207586493)

[3.9 AT+HOSTNAME 12](#_Toc207586494)

[3.9.1 Set the Device Hostname 12](#_Toc207586495)

[3.9.2 Query the Device Hostname 12](#_Toc207586496)

[3.10 AT+LOG\_LEVEL 12](#_Toc207586497)

[3.11 AT+PROTOCOL 14](#_Toc207586498)

[3.11.1 Set the Reporting Protocol for a Serial Interface 14](#_Toc207586499)

[3.11.2 Query the Reporting Protocol for All Serial Interfaces 14](#_Toc207586500)

[3.12 AT+REBOOT 14](#_Toc207586501)

[3.13 AT+RX\_ENABLE 15](#_Toc207586502)

[3.13.1 Enable or Disable the Receiver(s) 15](#_Toc207586503)

[3.13.2 Check Whether the Receiver(s) are Currently Enabled 15](#_Toc207586504)

[3.14 AT+SETTINGS 16](#_Toc207586505)

[3.14.1 Query Current Settings 16](#_Toc207586506)

[3.14.2 Dump Settings in AT Format 17](#_Toc207586507)

[3.14.3 Load Settings from EEPROM 17](#_Toc207586508)

[3.14.4 Save Settings to EEPROM 17](#_Toc207586509)

[3.14.5 Reset Settings to Factory Default 17](#_Toc207586510)

[3.15 AT+SUBG\_ENABLE 18](#_Toc207586511)

[1.1.1 Set Sub-GHz Receiver Enable Status and Line Drive Type 18](#_Toc207586512)

[1.1.2 Query Sub-GHz Receiver Enable Status and Line Drive Type 18](#_Toc207586513)

[3.16 AT+TEST 18](#_Toc207586514)

[3.17 AT+TL\_READ 19](#_Toc207586515)

[3.18 AT+TL\_OFFSET 19](#_Toc207586516)

[3.18.1 Set Trigger Level 19](#_Toc207586517)

[3.18.2 Query Trigger Level 19](#_Toc207586518)

[3.19 AT+UPTIME 20](#_Toc207586519)

[3.20 AT+WATCHDOG 20](#_Toc207586520)

[3.20.1 Configure the Watchdog Timer 20](#_Toc207586521)

[3.20.2 Query the Watchdog Timer 20](#_Toc207586522)

[3.20.3 Test the Watchdog Timer 20](#_Toc207586523)

[3.21 AT+WIFI\_AP 21](#_Toc207586524)

[3.21.1 Configure the WiFi Access Point 21](#_Toc207586525)

[3.21.2 Query the WiFi Access Point Configuration 21](#_Toc207586526)

[3.22 AT+WIFI\_STA 22](#_Toc207586527)

[3.22.1 Configure the WiFi Station 22](#_Toc207586528)

[3.22.2 Query the WiFi Station Configuration 22](#_Toc207586529)

[4 Reporting Protocols 23](#_Toc207586530)

[4.1 CSBee 24](#_Toc207586531)

[4.1.1 Mode S Aircraft Message 24](#_Toc207586532)

[4.1.2 UAT Aircraft Message 31](#_Toc207586533)

[4.1.3 Statistics Message 34](#_Toc207586534)

[4.2 GDL90 35](#_Toc207586535)

[4.3 MAVLINK 36](#_Toc207586536)

[4.3.1 MAVLINK\_HEARTBEAT （Message ID 0） Packet Definition 36](#_Toc207586537)

[4.3.2 MAVLINK ADSB\_VEHICLE (Message ID 246) Packet Definition 36](#_Toc207586538)

[4.3.3 MAVLINK\_REQUEST\_DATA\_STREAM (Message ID 66) Packet Definition 37](#_Toc207586539)

[4.3.4 MAVLINK MESSAGE\_INTERVAL (Message ID 244) Packet Definition 37](#_Toc207586540)

[4.4 Raw Packets 38](#_Toc207586541)

[4.4.1 Raw 1090MHz Mode S Frames 38](#_Toc207586542)

[4.4.2 Raw 978MHz UAT Frames 38](#_Toc207586543)

# Revision History

20250719

* Initial release with version control.

20250821

* Update CSBee protocol with new bit flag positions, new field for separate baro/GNSS vertical rates.
* Change AT+TL\_SET AT command to AT+TL\_OFFSET AT command.
* Change AT+PROTOCOL AT command to separate AT+PROTOCOL\_IN and AT+PROTOCOL\_OUT AT commands.

# Background

ADSBee 1090 was created as an attempt to build a low-cost ADS-B receiver without the use of an FPGA (found in most embedded ADS-B receivers on the market) and without the need for external compute (a requirement of most SDR-based ADS-B receivers). ADSBee 1090 accomplishes this through the use of a low-cost dual core microcontroller (RP2040) with flexible IO peripherals (PIO) that run a set of custom-written programs for preamble detection and packet decoding. By dedicating the RP2040’s PIO peripherals to the tasks required to find and decode ADS-B packets, ADSBee 1090 frees up its remaining cores to perform the logical functions required to validate checksums on decoded packets and decipher aircraft information (position, altitude, callsign, etc).

The ADSBee 1090 reports decoded aircraft information over UART and USB interfaces in a variety of protocols, and can utilize its attached ESP32 S3 module to host WiFi networks for data streaming to other devices, or connect to existing WiFi networks in order to upload data to the internet or other devices on the network.

Provisions are included for connecting an external GNSS module and UAT radio receiver to the ADSBee 1090. These features will enter development in the near future.

# Communication Interfaces

## Console Interface

The CONSOLE interface (USB-C connector) on the ADSBee 1090 can be used to supply the device with power, configure the device’s internal parameters via AT commands, and receive data from the device.

No baud rate configuration is necessary for the CONSOLE interface. Note that AT commands must be suffixed with CR+LF (“\r\n”) in order to be processed by the AT command parser.

## COMMS\_UART Interface

The COMMS\_UART interface is used for data output, and can support a number of different protocols. Data can be streamed out of the CONSOLE and COMMS\_UART interfaces simultaneously. The baud rate of the COMMS\_UART interface can be adjusted via AT commands.

**COMMS\_UART Parameters**

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Baud Rate | 115200 baud (default) |
| Data Bits | 8 |
| Stop Bits | 0 (N) |
| Parity Bits | 1 |
| Logic Level | 3.3V |

## GNSS\_UART Interface

The ADSBee 1090’s GNSS module connector includes a UART interface which can be used to receive NMEA sentences from a GNSS module. The baud rate of the GNSS\_UART interface can be adjusted via AT commands.

**GNSS\_UART Parameters**

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Baud Rate | 9600 baud (default) |
| Data Bits | 8 |
| Stop Bits | 0 (N) |
| Parity Bits | 1 |
| Logic Level | 3.3V |

# AT Commands

AT Commands are used to configure the ADSBee 1090 receiver’s internal parameters via the CONSOLE interface. AT commands can be used to set values (with the ‘=’ operator, e.g. “AT+BAUD\_RATE=COMMS\_UART,115200”) or query values (with the ‘?’ operator, e.g. “AT+BAUD\_RATE?”).

AT commands and parameters must be all-caps. Whitespace is not ignored and should only be used intentionally (e.g. as part of a WiFi network SSID which contains spaces). Arguments are separated by a single comma and no spaces.

All AT command arguments are optional. Arguments will be ignored if left as blank.For instance, to set the second parameter of AT+TL\_SET to 3000 without changing the value of the first parameter, the command “AT+TL\_SET=,3000” can be sent. Likewise, to change the first parameter to 2000 without changing the value of the second, the command “AT+TL\_SET=2000,” can be sent.

Commands from the user to the ADSBee 1090 are prefixed with “AT+” (e.g. “AT+BAUD\_RATE…”). Replies may be prefixed with the relevant command (e.g. “+BAUD\_RATE=…”) or nothing (e.g. “OK”). Replies to AT command queries may include text enclosed by parentheses (e.g. “AT+BAUD\_RATE=115200(COMMS),9600(GNSS). These text blobs are annotations to improve human readability of the reply.

|  |
| --- |
| **IMPORTANT NOTE**  No settings will be persisted after shutdown unless AT+SETTINGS=SAVE is executed in order to write new settings values to non-volatile storage. |

## AT+BAUD\_RATE

### Set Baud Rate

AT+BAUD\_RATE=<iface>,<baud\_rate>

Set the baud rate for a particular serial interface. Note that the USB C port (CONSOLE interface) is a virtual COM port and does not have a baud rate that can be changed.

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Description** | **Values** |
| iface | Serial interface to set the baud rate for. | COMMS\_UART, GNSS |
| baud\_rate | Baud rate, in characters per second. | 9600-115200 |

### Query Baud Rate

AT+BAUD\_RATE?

+BAUD\_RATE=<comms\_uart\_baud\_rate>(COMMS\_UART),<gnss\_uart\_baud\_rate>(GNSS\_UART)

Queries the baud rate for the COMMS\_UART and GNSS\_UART interfaces. Note that the baud rates returned by this query are the actual system baud rates, which should be close to the baud rates that were requested with AT+BAUDRATE but may be slightly different due to the particulars of how baud rates are implemented inside the RP2040.

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Description** | **Values** |
| comms\_uart\_baud\_rate | Baud rate on the COMMS\_UART interface. | 9600-115200 |
| gnss\_uart\_baud\_rate | Baud rate on the GNSS\_UART interface. | 9600-115200 |

## AT+BIAS\_TEE\_ENABLE

### Turn the Bias Tee On or Off

AT+BIAS\_TEE\_ENABLE=<enabled>

Enable or disable the bias tee to enable use of an external LNA.

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Description** | **Acceptable Values** |
| enabled | Whether the bias tee is enabled (3.3VDC supplied to the RF IN connector) or disabled (no DC voltage supplied to the RF IN connector). | 0 – Bias tee is disabled.  1 – Bias tee is enabled. |

### Query the Status of the Bias Tee

AT+BIAS\_TEE\_ENABLE?

+BIAS\_TEE\_ENABLE=<enabled>

Queries the status of the bias tee. See table in 3.1.1 for values and their meanings.

## AT+DEVICE\_INFO

Queries the device information of the ADSBee. An example query and reply is shown below.

|  |
| --- |
| > AT+DEVICE\_INFO?  Part Code: 010240002F-20240907-000001  RP2040 Firmware Version: 0.6.2  OTA Key 0: cf737c4fce892fab44c6ec0d5d0f66dccf06c5630ac5b531f4067599df014d5ef213bb73205a9ce378318f259e3d01e3b99c089a75ac0735b204256b9371fbce  OTA Key 1: 1701a736dc40c837f318c9e7ae82557a39fe07588d3745602bb9269b13843b87ca7962daecc9897c6dfb0ac4ec77997e9cc34cd356e415fc46eb4ae3dd42b717  ESP32 Firmware Version: 0.6.2  ESP32 Base MAC Address: 64:E8:33:5D:0B:C4  ESP32 WiFi Station MAC Address: 64:E8:33:5D:0B:C4  ESP32 WiFi AP MAC Address: 64:E8:33:5D:0B:C5  ESP32 Bluetooth MAC Address: 64:E8:33:5D:0B:C6  ESP32 Ethernet MAC Address: 64:E8:33:5D:0B:C7 |

## AT+ESP32\_ENABLE

### Turn the ESP32 On or Off

AT+ESP32\_ENABLE=<enabled>

Turns the ESP32 on or off using its enable line. When the ESP32 is turned off, the ADSBee 1090 will draw less power, but the WiFi and network capabilities will be unavailable. This operational mode is useful for conserving energy in applications where the ADSBee is only being communicated with via its serial interfaces.

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Description** | **Acceptable Values** |
| enabled | Whether the ESP32 is turned on. | 0 – ESP32 is turned on.  1 – ESP32 is turned off. |

### Query the Status of the ESP32

AT+ESP32\_ENABLE?

+ESP32\_ENABLE=<enabled>

Queries whether the ESP32 is turned on or off. See table in 3.4.1 for the values and their meanings.

## AT+ESP32\_FLASH

AT+ESP32\_FLASH

Flashes the ESP32 with the firmware image stored on the RP2040. This should never be needed, since the RP2040 does a firmware version check of the ESP32 on startup and automatically reflashes he firmware if it is out of date. The AT+ESP32\_FLASH command is only used in weird debugging scenarios where the version number of the firmware on the ESP32 matches the version of the firmware stored on the RP2040, but the firmware stored on the RP2040 is different and needs to be flashed onto the ESP32.

## AT+ETHERNET

### Enable or Disable Ethernet

Enables or disables Ethernet functionality on the ESP32. Must be connected to a W5500 Ethernet IC via SPI.

AT+ETHERNET=<enabled>

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Description** | **Acceptable Values** |
| enabled | Whether Ethernet connectivity is enabled via the ESP32 and a connected W5500 Ethernet IC. | 0 – Ethernet is enabled.  1 – Ethernet is disabled. |

### Query Ethernet Setting

AT+ETHERNET?

+ETHERNET=1

## AT+FEED

### Configure a Feed

AT+FEED=<index>,<uri>,<port>,<active>,<protocol>

Example command for configuring feed 0 to send data to airplanes.live, which accepts Mode S Beast protocol on port 30004 at the static IP 78.46.234.18:

AT+FEED=0,78.46.234.18,30004,1,BEAST

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Description** | **Acceptable Values** |
| index | Which feed slot to configure. | 0-5 |
| uri | Static IP address or hostname of the feed destination. If the field is given as a hostname, a DNS lookup will be performed in order to convert the hostname to an IP address. | Public IP address, e.g. 78.46.234.18  Hostname, e.g. feed.whereplane.xyz  Maximum length 64 characters. |
| port | Port number to feed to. | 0-65535 |
| active | Whether the feed should be activated. This can be used to temporarily disable a feed while still keeping its configuration information intact. | 0 – Feed is active.  1 – Feed is disabled. |
| protocol | Which protocol to use when feeding. | BEAST – Send validated packets in Mode S Beast format.  BEAST\_RAW – Send both validated and invalid (bad checksum) packets in Mode S Beast format. |

### Query Configuration of All Feeds

AT+FEED?

+FEED=0(INDEX),192.168.1.103(URI),30004(PORT),1(ACTIVE),BEAST(PROTOCOL),bee00038172d18c(RECEIVER\_ID)

+FEED=1(INDEX),(URI),0(PORT),0(ACTIVE),NONE(PROTOCOL),bee00038172d18c(RECEIVER\_ID)

+FEED=2(INDEX),(URI),0(PORT),0(ACTIVE),NONE(PROTOCOL),bee00038172d18c(RECEIVER\_ID)

+FEED=3(INDEX),(URI),0(PORT),0(ACTIVE),NONE(PROTOCOL),bee00038172d18c(RECEIVER\_ID)

+FEED=4(INDEX),78.46.234.18(URI),30004(PORT),1(ACTIVE),BEAST(PROTOCOL),bee00038172d18c(RECEIVER\_ID)

+FEED=5(INDEX),feed.whereplane.xyz(URI),30004(PORT),0(ACTIVE),BEAST(PROTOCOL),bee00038172d18c(RECEIVER\_ID)

### Query Configuration of a Single Feed

AT+FEED?<index>

Example query for configuration of feed 0 only:

AT+FEED?0

+FEED=0(INDEX),192.168.1.103(URI),30004(PORT),1(ACTIVE),BEAST(PROTOCOL),bee00038172d18c(RECEIVER\_ID)

## AT+HELP

AT+HELP

AT Command Help Menu:

+BAUDRATE:

AT+BAUDRATE=<iface>,<baudrate>

Set the baud rate of a serial interface.

AT\_BAUDRATE?

Query the baud rate of all serial interfaces.

+BIAS\_TEE\_ENABLE:

AT+BIAS\_TEE\_ENABLE=<enabled>

Enable or disable the bias tee.

BIAS\_TEE\_ENABLE?

Query the status of the bias tee.

...

Prints the available AT commands as well as how to use them. The list of commands in the preview above is abridged.

## AT+HOSTNAME

### Set the Device Hostname

AT+HOSTNAME=<hostname>

Sets the device hostname, which can make things easier when configuring a local network. Hostname is also used for mDNS, allowing you to visit the device’s webpage at <hostname>.local.

### Query the Device Hostname

AT+HOSTNAME?

+HOSTNAME=ADSBee1090-0240907000001

## AT+LOG\_LEVEL

AT+LOG\_LEVEL=<log\_level>

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Description** | **Acceptable Values** |
| log\_level | Log verbosity level for the console. Anything being printed with a lower verbosity than the specified level will be suppressed. A verbosity level of AT+LOG\_LEVEL=WARNINGS is recommended.  Terminal prints are color coded on the Serial CLI (but not on the Web CLI). Errors are printed in red, warnings are printed in yellow, and other prints have no color coding. | INFO – Informational logs. Details every packet received by the ADSBee and whether it passed checksum. Also prints all warnings and errors.  WARNINGS – Warning logs. Prints out every time something unexpected happens. Warnings include recoverable errors and unexpected values encountered within ADS-B packets being decoded. Also prints all errors.  ERRORS – Error logs. Prints every time there is a severe error, such as packets being lost in communication between the RP2040 and ESP32, a peripheral failing to communicate properly, or fatal errors in code.  SILENT – No logs. Only AT command replies and console protocols will be printed. Use this setting to avoid having log messages injected into the console text stream if it is being used to report a protocol to another device. |

## AT+PROTOCOL\_OUT

### Set the Reporting Protocol for a Serial Interface

AT+PROTOCOL\_OUT=<iface>,<protocol>

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Description** | **Values** |
| iface | Serial interface to set the baudrate for. | CONSOLE, COMMS\_UART |
| protocol | Reporting protocol for the specified serial interface | NONE – No data reported.  RAW – Raw plain text reporting protocol.  BEAST – Mode S Beast binary reporting protocol.  CSBEE – CSBEE plain text reporting protocol.  MAVLINK1 – MAVLINK 1 binary reporting protocol. MAVLINK2 – MAVLINK 2 binary reporting protocol.  GDL90 – Garmin GDL90 binary reporting protocol. |

### Query the Reporting Protocol for All Serial Interfaces

AT+PROTOCOL\_OUT?

+PROTOCOL\_OUT=CONSOLE,<console\_protocol>

+PROTOCOL\_OUT=COMMS\_UART,<comms\_uart\_protocol>

Queries the reporting protocol set for each of the serial interfaces. See the table in 3.11.1 for protocol definitions.

## AT+REBOOT

AT+REBOOT

Reboots the ADSBee 1090 immediately.

## AT+RX\_ENABLE

### Enable or Disable the Receiver(s)

AT+RX\_ENABLE=<all\_enabled>,<1090\_enabled>,<subg\_enabled>

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Description** | **Values** |
| all\_enabled | Flag indicating whether to ignore 1090\_enabled and subg\_enabled flags and enable / disable all radios. | 1 – All radios enabled.  0 – All radios disabled. |
| 1090\_enabled | Flag indicating whether the 1090MHz receiver should be enabled or disabled.  NOTE: Disabling the 1090MHz receiver does not conserve any power, as the RF frontend is still active. This receiver disable flag simply disables an interrupt within the RP2040 that is used to check for incoming transponder messages. | 1 – 1090MHz receiver is enabled.  0 – 1090MHz receiver is disabled. |
| subg\_enabled | Flag indicating whether the Sub-GHz receiver should be enabled or disabled (if equipped).  Disabling the Sub-GHz receiver does save a small amount of power, as the Sub-GHz transceiver chip will be powered down. | 1 – Sub-GHz receiver is enabled.  0 – Sub-GHz receiver is disabled. |

### Check Whether the Receiver(s) are Currently Enabled

AT+RX\_ENABLE?

1090 Receiver: ENABLED

SubG Receiver: DISABLED

## AT+SETTINGS

### Query Current Settings

AT+SETTINGS?

Settings Struct

Receiver: ENABLED

Trigger Level: 1300 milliVolts (-62 dBm)

Bias Tee: DISABLED

Watchdog Timeout: 10 seconds

Log Level: WARNINGS

Reporting Protocols:

CONSOLE: NONE

COMMS\_UART: CSBEE

Comms UART Baud Rate: 115207 baud

GNSS UART Baud Rate: 9600 baud

ESP32: ENABLED

WiFi AP: ENABLED

Channel: 3

SSID: ADSBee1090-0240907000001

Password: yummyflowers

WiFi STA: ENABLED

SSID: Smart Bidet Wifi

Password: \*\*\*\*\*\*\*\*

Feed URIs:

0 URI:192.168.1.103 Port:30004 ACTIVE Protocol:BEAST ID:0xbee00038172d18c1

1 URI: Port:0 INACTIVE Protocol:NONE ID:0xbee00038172d18c1

2 URI: Port:0 INACTIVE Protocol:NONE ID:0xbee00038172d18c1

3 URI: Port:0 INACTIVE Protocol:NONE ID:0xbee00038172d18c1

4 URI:78.46.234.18 Port:30004 ACTIVE Protocol:BEAST ID:0xbee00038172d18c1

5 URI:feed.whereplane.xyz Port:30004 INACTIVE Protocol:BEAST ID:0xbee00038172d18c1

OK

### Dump Settings in AT Format

Sending AT+SETTINGS?DUMP outputs a dump of all nonvolatile settings in AT command format, allowing them to be easily re-entered when restoring the ADSBee settings after a firmware upgrade, or for moving setting between devices.

AT+SETTINGS?DUMP

AT+SETTINGS=RESET

AT+BAUD\_RATE=CONSOLE,115200

AT+BAUD\_RATE=COMMS\_UART,115200

AT+BAUD\_RATE=GNSS\_UART,115200

AT+BIAS\_TEE\_ENABLE=0

AT+ESP32\_ENABLE=1

AT+FEED=0,,0,0,NONE

AT+FEED=1,,0,0,NONE

AT+FEED=2,,0,0,NONE

AT+FEED=3,,0,0,NONE

AT+FEED=4,feed.airplanes.live,30004,1,BEAST

AT+FEED=5,feed.adsb.fi,30004,1,BEAST

AT+LOG\_LEVEL=WARNINGS

AT+PROTOCOL=CONSOLE,NONE

AT+PROTOCOL=COMMS\_UART,MAVLINK1

AT+RX\_ENABLE=1

AT+TL\_SET=1300

AT+WATCHDOG=10

AT+WIFI\_AP=1,ADSBee1090-0240907000001,yummyflowers,11

AT+WIFI\_STA=0,,

OK

### Load Settings from EEPROM

AT+SETTINGS=LOAD

### Save Settings to EEPROM

AT+SETTINGS=SAVE

Note that this command is also used to synchronize settings between the RP2040 and ESP32. When changing parameters in the Serial CLI or Web CLI, run AT+SETTINGS=SAVE or reboot the device to synchronize new settings (e.g. new feed parameters or network settings).

### Reset Settings to Factory Default

AT+SETTINGS=RESET

Note that this command resets settings to factory defaults, but will not persist them to the next power on unless AT+SETTINGS=SAVE is run subsequently.

## AT+SUBG\_ENABLE

Enable or disable the Sub-GHz receiver, if present. Can be used to drive the Sub-GHz receiver enable line HI or LO, or leave the corresponding GPIO in a high impedance state in order to allow external control (e.g. for using an external debugger).

### Set Sub-GHz Receiver Enable Status and Line Drive Type

AT+SUBG\_ENABLE=<enabled>

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Description** | **Values** |
| enabled | Flag indicating whether the Sub-GHz receiver should be enabled or disabled. | 0 – Sub-GHz receiver is disabled.  1 – Sub-GHz receiver is enabled.  EXTERNAL – Sub-GHz receiver enable is pulled low by default, but can be overridden by an external device. |

### Query Sub-GHz Receiver Enable Status and Line Drive Type

AT+SUBG\_ENABLE?

+SUBG\_ENABLE=1

## AT+TEST

Used for running internal self-tests. Can only be run once per boot cycle.

AT+TEST

[==========] Running 4 test cases.

[ RUN ] SpiCoprocessor.WriteReadScratchNoAck

[ OK ] SpiCoprocessor.WriteReadScratchNoAck (687000ns)

[ RUN ] SpiCoprocessor.WriteReadScratchWithAck

[ OK ] SpiCoprocessor.WriteReadScratchWithAck (751000ns)

[ RUN ] SPICoprocessor.ReadWriteReadRewriteRereadBigNoAck

[ OK ] SPICoprocessor.ReadWriteReadRewriteRereadBigNoAck (25336000ns)

[ RUN ] SPICoprocessor.ReadWriteReadRewriteRereadBigWithAck

[ OK ] SPICoprocessor.ReadWriteReadRewriteRereadBigWithAck (29287000ns)

[==========] 4 test cases ran.

[ PASSED ] 4 tests.

## AT+TL\_READ

AT+TL\_READ?

+TL\_READ=1258mV (-64 dBm)

Queries the current value of the internal trigger level of the RF frontend’s data slicer circuit. Signals peaking above this level will trigger a demodulation. This value should be set substantially above the noise floor in order to avoid false triggers.

Note that the value returned from TL\_READ is different from querying TL\_SET, since the value returned by TL\_READ is read from the RP2040’s ADC, while the value returned from querying TL\_SET is the setpoint for the PWM output that generates the trigger level signal. They should be roughly similar, but slightly offset.

## AT+TL\_OFFSET

### Set Trigger Level

AT+TL\_OFFSET=<command>

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Description** | **Values** |
| command | Trigger level offset (milliVolts above the measured noise floor), or the activation word to begin a self-learning process for the trigger level using simulated annealing. | 0-3300  LEARN  Trigger level defaults to 200. |

The AT+TL\_OFFSET command sets the value of the internal trigger level of the RF frontend’s data slicer circuit. Signals peaking above this level will trigger a demodulation. This value should be set above the noise floor in order to avoid false triggers.

A higher trigger level makes the receiver less sensitive, while a lower trigger level makes the receiver more sensitive (and thus more likely to be triggered by unwanted noise).

A self-learning process can be activated by sending AT+TL\_OFFSET=LEARN instead of providing a trigger value in milliVolts. The self-learning process uses simulated annealing, where a random trigger value is chosen, and then random neighbors are traversed to if their trigger levels seem to provide an improved number of valid packets within the learning window. The allowable traversal distance is gradually decreased over time until a final value is settled upon. The self-learning process takes approximately 20 minutes. Note that as of the current firmware revision, hand-tuning the trigger value (or using the provided default value) may outperform the self-learning routine.

### Query Trigger Level

AT+TL\_OFFSET?

+TL\_OFFSET=200mV

Queries the trigger level that is set internally. Note that this may differ from the actual value that is read using an ADC, as provided by AT+TL\_READ.

## AT+UPTIME

Queries the uptime of the ADSBee, in seconds.

AT+UPTIME?

+UPTIME=71

## AT+WATCHDOG

The ADSBee features a watchdog timer on the RP2040, which will automatically reset all microcontrollers on the board if code executing on the RP2040 freezes up, or if SPI communication with the ESP32 breaks down. This is intended to provide a means of automatic recovery in case of a hard fault caused by firmware bugs (likely), power glitches (maybe), or cosmic rays (probably not). As the watchdog may not be wanted in some cases, like debugging hardfaults, or during device programming / beakpoint debugging, it can be disabled. Additionally, means are provided for self-testing the watchdog via AT command in order to verify that it is still active.

### Configure the Watchdog Timer

AT+WATCHDOG=<timeout\_sec>

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Description** | **Values** |
| command | Trigger level, in milliVolts, or the activation word to begin a self-learning process for the trigger level using simulated annealing. | 0-3300  LEARN |

### Query the Watchdog Timer

AT+WATCHDOG?

+WATCHDOG=10

Prints the value of the watchdog timer in seconds, or 0 if the watchdog timer is disabled.

### Test the Watchdog Timer

AT+WATCHDOG=TEST

Blocking for 11 seconds.

(ADSBee Reboots here)

The AT+WATCHDOG=TEST command blocks the processor for the currently configured watchdog timeout plus one second. This should induce a device reboot, otherwise an error message will be displayed indicating that the watchdog failed to activate.

## AT+WIFI\_AP

The ADSBee creates its own WiFi access point that allows other devices to join its network in order to access the Web CLI and receive aircraft data (e.g. GDL90 traffic info over UDP port 4000). The WiFi AP can be enabled/disabled and can have its SSID, password, and WiFi channel customized. Note that WiFi settings don’t have any affect unless the ESP32 is enabled, and are not propagated to the ESP32 unless settings are saved with AT+SETTINGS=SAVE.

### Configure the WiFi Access Point

AT+WIFI\_AP=<enabled>,<ap\_ssid>,<ap\_pwd>,<ap\_channel>

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Description** | **Values** |
| enabled | Toggle whether the AP is enabled or disabled. | 0 – Disable WiFi access point.  1 – Enable WiFi access point. |
| ap\_ssid | SSID for the access point. Defaults to a unique SSID with the format “ADSBee1090-0240907000001”. Can be set to a value up to 32 characters long. | ASCII string up to 32 characters in length. |
| ap\_pwd | Password for the access point. Defaults to “yummyflowers”. Can be set to a value up to 64 characters long. | ASCII string up to 64 characters in length. |
| ap\_channel | WiFi channel number for the access point. Can be set to a value from 1-11. A random channel value is chosen by default during initial programming of the device. It is recommended to change the channel value to a frequency with low utilization in the installation location. | 1-11 |

### Query the WiFi Access Point Configuration

AT+WIFI\_AP?

+WIFI\_AP=1,ADSBee1090-0240907000001,yummyflowers,3

Reply format matches argument values and ordering from the configuration command.

## AT+WIFI\_STA

The ADSBee can join external WiFi networks as a WiFi station in order to allow connections from other devices on the existing network, or to connect to the internet in order to feed remote endpoints with air traffic data.

### Configure the WiFi Station

AT+WIFI\_STA=<enabled>,<sta\_ssid>,<sta\_pwd>

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Description** | **Values** |
| enabled | Toggle whether the AP is enabled or disabled. | 0 – Disable WiFi station.  1 – Enable WiFi station. |
| sta\_ssid | SSID for the access point to connect to. Can be set to a value up to 32 characters long. | ASCII string up to 32 characters in length. |
| sta\_pwd | Password for the access point to connect to. Can be set to a value up to 64 characters long. | ASCII string up to 64 characters in length. |

### Query the WiFi Station Configuration

+WIFI\_STA=1,My Supercool WiFi Network,\*\*\*\*\*\*\*\*\*\*

Queries the configuration used by the ADSBee to join an external WiFi network. Note that the value and ordering of the arguments is identical to the configuration command, except the password is censored.

# Reporting Protocols

ADSBee 1090 supports the following reporting protocols on CONSOLE and COMMS\_UART.

* CSBee
* GDL90
* MAVLINK 1
* MAVLINK 2
* Mode S Beast
* Raw Packets

The CONSOLE interface reports debug messages and AT command responses in addition to the selected reporting protocol. If the CONSOLE interface is being used as a reporting interface, it is recommended to send AT+LOG\_LEVEL=SILENT to silence any debug logs that might corrupt the reported data, and to avoid sending additional AT commands while reading reported data in order to avoid the reported data being interspersed with OK and other AT command responses from the ADSBee 1090.

## CSBee

Comma Separated Bee protocol containing information about tracked aircraft as plain text.

The CSBee protocol is heavily inspired by the Aerobits Aero CSV protocol.

### Mode S Aircraft Message

This message contains information about an aircraft being tracked via ADS-B (1090MHz). Aircraft reports are provided once per second, per aircraft, until contact with the aircraft has been lost for 60 seconds.

#A:ICAO,FLAGS,CALL,SQUAWK,ECAT,LAT,LON,BARO\_ALT,GNSS\_ALT,DIR,SPEED,BARO\_VRATE,GNSS\_VRATE,NICNAC,ACDIMS,VERSION,SIGS,SIGQ,SFPS,ESFPS,CRC\r\n

|  |  |  |  |
| --- | --- | --- | --- |
| **Field** | **Description** | **Format** | **Example value** |
| #A | Mode S aircraft message start indicator. |  |  |
| ICAO | ICAO number of aircraft (3 bytes). | Hex Integer | 3C65AC |
| FLAGS | Flags bitfield, see table 4.1.1.1. | Hex Integer | 12F356A8 |
| CALL | Callsign of aircraft. | String | N61ZP |
| SQUAWK | SQUAWK of aircraft. | Octal Integer | 7232 |
| ECAT | Emitter category, see table 4.1.1.2. | Integer | 14 |
| LAT | Latitude, in degrees. | Float | 57.57634 |
| LON | Longitude, in degrees. | Float | 17.59554 |
| BARO\_ALT | Barometric altitude, in feet. | Integer | 5000 |
| GNSS\_ALT | Geometric altitude, in feet. | Integer | 5000 |
| DIR | Direction of aircraft, in degrees [0,360). Consult bit flags to determine whether this field is true heading, magnetic heading, or track. | Integer | 35 |
| SPEED | Horizontal velocity of aircraft, in knots. | Integer | 464 |
| BARO\_VRATE | Barometric vertical velocity of aircraft, in ft/min. | Integer | -1344 |
| GNSS\_VRATE | Geometric vertical velocity of the aircraft, in ft/min | Integer | -1344 |
| NICNAC | Aircraft data integrity. See table 4.1.1.3 | Hex Integer |  |
| ACDIMS | Aircraft physical dimensions and system design assurance. See table 4.1.1.4. | Hex Integer | 31BE89F2 |
| VERSION | ADS-B protocol version used by the aircraft. | Integer | 2 |
| SIGS | Signal strength, in dBm. | Integer | -92 |
| SIGQ | Signal quality, in dB. | Integer | 2 |
| SFPS | Number of valid 56-bit Squitter Mode S frames received from the aircraft during the last second. | Integer | 2 |
| ESFPS | Number of valid 112-bit Extended Squitter Mode S frames received from the aircraft during the last second. | Integer | 5 |
| CRC | CRC16 (described in 4.1.1.5). | Hex Integer | 2D3E |

#### FLAGS Bitfield

Note: All bits 25-31 are momentary (cleared and updated every reporting interval).

|  |  |  |
| --- | --- | --- |
| **Bit** | **Bit Name** | **Meaning if the bit is set (1)** |
| 0 | IS\_AIRBORNE | Emitter is airborne. |
| 1 | BARO\_ALTITUDE\_VALID | Emitter has provided a barometer altitude. |
| 2 | GNSS\_ALTITUDE\_VALID | Emitter has provided a GNSS altitude. |
| 3 | POSITION\_VALID | Emitter has provided a pair of even and odd Compact Position Reporting packets that were decoded to a location. |
| 4 | DIRECTION\_VALID | Emitter has provided a direction (may be ground track, magnetic compass heading, or true compass heading). |
| 5 | HORIZONTAL\_SPEED\_VALID | Emitter has provided a horizontal velocity. |
| 6 | BARO\_VERTICAL\_RATE\_VALID | Emitter has provided a barometric vertical velocity. |
| 7 | GNSS\_VERTICAL\_RATE\_VALID | Emitter has provided a GNSS vertical velocity. |
| 8 | IS\_MILITARY | Emitter has transmitted at least one packet using a military format, such as Military Extended Squitter (DF=19). |
| 9 | IS\_CLASS\_B2\_GROUND\_VEHICLE | Emitter is actually a ground vehicle using a Class B2 transponder with a transmission power < 70W. |
| 10 | HAS\_1090\_ES\_IN | Emitter has receive capability for 1090MHz Extended Squitter transmissions. |
| 11 | HAS\_UAT\_IN | Emitter has receive capability for UAT (978MHz Universal Access Transceiver) transmissions. |
| 12 | TCAS\_OPERATIONAL | Emitter has a functional TCAS (Traffic Collision Avoidance System) onboard. |
| 13 | SINGLE\_ANTENNA | Emitter is using a single antenna, instead antennas above and below the fuselage. Transmissions may be weak or irregular during maneuvering. |
| 14 | DIRECTION\_IS\_HEADING | Surface position messages provided by the aircraft indicate a heading and not a track angle. |
| 15 | HEADING\_USES\_MAGNETIC\_NORTH | Heading reported by the aircraft while on the surface uses magnetic north instead of true north. |
| 16 | IDENT | The aircraft has its SPI (Special Position Identification) bits set in Mode A/C or Mode S messages. This indicates that the pilot has depressed the momentary IDENT switch on their transponder, most likely at the request of air traffic control. |
| 17 | ALERT | The aircraft is issuing either a permanent or momentary alert. This could correspond to an operational mode change or something else. |
| 18 | TCAS\_RA | The aircraft has an active TCAS resolution advisory (i.e. the aircraft is warning the pilot to take action in order to avoid colliding with another aircraft). |
| 19-22 Reserved | | |
| 23 | UPDATED\_BARO\_ALTITUDE | Barometric altitude has been updated within the last reporting interval. |
| 24 | UPDATED\_GNSS\_ALTITUDE | GNSS altitude has been updated within the last reporting interval. |
| 25 | UPDATED\_POSITION | Position (latitude / longitude) has been updated within the last reporting interval. |
| 26 | UPDATED\_DIRECTION | Direction has been updated within the last reporting interval. |
| 27 | UPDATED\_HORIZONTAL\_SPEED | Horizontal velocity has been updated within the last reporting interval. |
| 28 | UPDATED\_BARO\_VERTICAL\_RATE | Barometric vertical velocity has been updated within the last reporting interval. |
| 29 | UPDATED\_GNSS\_VERTICAL\_RATE | GNSS vertical velocity has been updated within the last reporting interval. |
| 30-31 Reserved | | |

#### ECAT Field

The ECAT field indicates the Emitter Category (i.e. airframe type) for each ADSB emitter that is being tracked. This field contains information about what kind of aircraft, ground vehicle, obstacle, or other airspace user is emitting ADS-B packets, and can be used to understand the emitter’s maneuvering capability and potential for wake vortex impact.

|  |  |
| --- | --- |
| **ECAT Value** | **Emitter Category** |
| -1 | Invalid |
| 0 | No Category Information |
| 1 | Light Aircraft (< 7,000kg) |
| 2 | Medium 1 (7,000kg – 34,000kg) |
| 3 | Medium 2 (34,000kg – 136,000kg) |
| 4 | High Vortex Aircraft |
| 5 | Heavy (> 136,000kg) |
| 6 | High Performance (> 5 G acceleration and > 400 kts speed) |
| 7 | Rotorcraft |
| 8 | Reserved |
| 9 | Glider / Sailplane |
| 10 | Lighter Than Air |
| 11 | Parachutist / Skydiver |
| 12 | Ultralight / Hang Glider / Paraglider |
| 13 | Reserved 1 |
| 14 | Unmanned Aerial Vehicle |
| 15 | Space / Transatmospheric Vehicle |
| 16 | Reserved 2 |
| 17 | Surface Emergency Vehicle |
| 18 | Surface Service Vehicle |
| 19 | Point Obstacle |
| 20 | Cluster Obstacle |
| 21 | Line Obstacle |

#### 

#### NICNAC Bitfield

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **NICNAC Bitfield** | | | | | | | | | | | | | | | |
| 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| Source Integrity Level (SIL) | | Geometric Vertical Accuracy (GVA) | | Navigation Accuracy Category: Position (NACp) | | | | Navigation Accuracy Category: Velocity (NACv) | | | Navigation Integrity Category: Barometer (NICbaro) | Navigation Integrity Category (NIC) | | | |

**NICNAC[0-3]: Navigation Integrity Category (NIC)**

The radius of containment (NIC) indicates how much trust should be placed in an aircraft’s reported location in the horizonal plane. The NIC reports a radius of containment specified by the avionics system of the emitter. The probability that the aircraft is outside of this radius of containment due to its avionics system receiving a faulty signal from one of its inputs (without displaying an error) is provided by another bitfield called the Source Integrity Level (SIL). Combined, the NIC and SIL indicate how likely it is that an aircraft is not actually contained by a bubble of a specified size, centered at the aircraft’s reported location, assuming that the avionics onboard the aircraft are functioning correctly but may be given faulty inputs.

A higher NIC value indicates more trust in an aircraft’s reported latitude / longitude position.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **NIC­ Value** | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 |
| **Radius of Containment** | Unknown | < 20 NM | < 8 NM | < 4 NM | < 2 NM | < 1 NM | < 0.6 NM | < 0.2 NM | < 0.1 NM | < 75 m | < 25 m | < 7.5 m |

#### NICNAC [4]: Navigation Integrity Category: Barometer (NICbaro)

The barometric altitude integrity (NICbaro) indicates how much trust should be placed in an aircraft’s reported altitude. The field is a single bit that indicates whether the aircraft uses an altimeter that has been cross-checked against other sources. Old school encoding altimeters have many parallel wires and output an altitude in a format called a Gillham Code, and have no built-in method of error checking. A single faulty wire can result in erroneous readings, so this bit lets air traffic control know whether to take altitude readings from the aircraft with a grain of salt. A 0 indicates that the transponder is outputting altitude from a Gillham coded source (with no way to cross check the value), while a 1 indicates that the transponder is outputting altitude from a Gillham coded source while using another sensor to cross-check it, or is using a more modern barometer that supports a protocol with built-in error checking.

A higher NICbaro value (i.e. 1 instead of 0) indicates more trust in the aircraft’s reported altitude.

|  |  |  |
| --- | --- | --- |
| **NICbaro Value** | 0 | 1 |
| **Barometric Altitude Integrity** | Altitude is from a Gillham-coded input, not cross checked. | Altitude is from a Gillham-coded input that is being cross-checked with another source, or from a non Gillham-coded input with built-in error checking features. |

#### NICNAC [5-7]: Navigation Accuracy Category: Velocity (NACv)

The horizontal velocity error (NACv) indicates the expected accuracy of the reported velocity of the aircraft when systems are operating nominally. This varies depending on the accuracy capabilities of the measurement equipment onboard the aircraft, and not how often we expect said equipment to fail.

A higher NACv indicates a more accurate velocity measurement system.

|  |  |
| --- | --- |
| **NACv Value** | **Horizontal Velocity Error** |
| 0b000 | Unknown or ≥ 10 m/s |
| 0b110 | < 10 m/s |
| 0b010 | < 3 m/s |
| 0b011 | < 1 m/s |
| 0b100 | < 0.3 m/s |

#### NICNAC [8-11]: Navigation Accuracy Category: Position (NACp)

The estimated position uncertainty (NACp) indicates the expected accuracy of the aircraft’s reported location when systems are operating nominally. This varies depending on the capabilities of the aircraft’s positioning system and not on how often we expect said equipment to fail.

A higher NACp indicates a more accurate positioning system.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **NACp Value** | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 |
| **Estimated Position Uncertainty** | Unknown or ≥ 10NM | < 10 NM | < 4 NM | < 2 NM | < 1 NM | < 0.5 NM | < 0.3 NM | < 0.1 NM | < 0.5 NM | < 30 m | < 10 m | < 3 m |

#### NICNAC[12-13]: Geometric Vertical Accuracy (GVA)

The geometric vertical accuracy indicates the 95% confidence interval (vertical figure of merit) provided by the aircraft’s onboard GNSS system (i.e. assuming some distribution of altitudes, the aircraft’s GNSS system is confident that 95 out of 100 times, the aircraft falls within some height of the reported geometric altitude.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **GVA Value** | 0 | 1 | 2 | 3 |
| **95% Vertical Figure of Merit (VFOM)** | Unknown or ≥ 150 m | < 150 m | ≤ 45 m | < 45 m (Was previously “reserved”, the actual value of this field may change but is guaranteed to be < 45 m). |

#### NICNAC[14-15]: Source Integrity Level (SIL)

The source integrity level indicates the probability that the aircraft exceeds the bounds of its horizontal radius of containment (NIC) due to a silent fault in signals received by the aircraft (no avionics failure).

|  |  |
| --- | --- |
| **SIL Value** | **Probability of Exceeding NIC Radius of Containment Due to Silent Fault** |
| 0 | Unknown or > 1x10-3 per flight hour. |
| 1 | ≤ 1x10-3 per flight hour. |
| 2 | ≤ 1x10-5 per flight hour. |
| 3 | ≤ 1x10-7 per flight hour. |
| 4 | Unknown or > 1x10-3 per sample. |
| 5 | ≤ 1x10-3 per sample. |
| 6 | ≤ 1x10-5 per sample. |
| 7 | ≤ 1x10-7 per sample. |

#### ACDIMS Bitfield

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **ACDIMS Bitfield** | | | | | | | | | | | | | | | |
| 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 |
| GNSS Offset Forward of Reference Point  (GOF) | | | | | | | | GNSS Offset Right of Reference Point  (GOR) | | | | | | | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| Aircraft Length  (ACL) | | | | | | | Aircraft Width  (ACW) | | | | | | | System Design Assurance (SDA) | |

**ACDIMS[0-1]: System Design Assurance (SDA)**

The system design assurance indicates how robust the aircraft’s position reporting systems are to failures of various severities. For instance, SDA = 1, a low SDA value, corresponds to Software and Hardware Design Assurance Level D, which states that a minor failure could cause the aircraft to transmit misleading position information with a probability of ≤ 1x10-3 per flight hour. A more robust system with SDA = 3, corresponding to Software and Hardware Design Assurance Level B, is expected to transmit misleading position information with a probability of 1x10-7 per flight hour even under a Hazardous failure condition.

Software Design Assurance categories used in this field are classified under RTCA DO-178B, Airborne Electronic Hardware Design Assurance are classified under RTCA DO-254, and failure classification levels are defined in FAA Advisory Circular [AC-23.1309-1E](https://www.faa.gov/regulations_policies/advisory_circulars/index.cfm/go/document.information/documentID/1019681).

|  |  |  |  |
| --- | --- | --- | --- |
| **SDA Value** | **Supported Failure Condition** | **Probability of Undetected Fault causing transmission of False or Misleading Information** | **Software and Hardware Design Assurance Level** |
| 0 | Unknown / No Safety Effect | > 1x10-3 per flight hour or unknown. | N/A |
| 1 | Minor | ≤ 1x10-3 per flight hour. | D |
| 2 | Major | ≤ 1x10-5 per flight hour. | C |
| 3 | Hazardous | ≤ 1x10-7 per flight hour. | B |

**ACDIMS[2-8] Aircraft Width (ACW)**

Approximate value for the width of the aircraft bounding box, in meters. Can be interpreted as a 7-bit unsigned integer.

**ACDIMS[9-15] Aircraft Length (ACL)**

Approximate value for the length of the aircraft bounding box, in meters. Can be interpreted as a 7-bit unsigned integer.

**ACDIMS[16-23] GNSS Offset Right of Reference Point (GOR)**

Signed 8-bit integer representing the left/right offset of the GNSS antenna from the aircraft’s reference point. A positive value indicates that the GNSS antenna is to the right of the aircraft reference point.

**ACDIMS[24-31] GNSS Offset Forward of Reference Point (GOF)**

Signed 8-bit integer representing the forward/back offset of the GNSS antenna from the aircraft’s reference point. A positive value indicates that the GNSS antenna is forward of the aircraft’s reference point. Always 0 for Mode S aircraft.

#### CRC Field

#### CSBee messages use a 16-bit Cyclical Redundancy Checksum (CRC-16), which can be calculated using the algorithm in the C++ code snippet below. Note the “swap16” helper function which also needs to be included.

uint16\_t swap16(uint16\_t value) { return (value << 8) | (value >> 8); }

uint16\_t CalculateCRC16(const uint8\_t \*data\_p, int32\_t length) {

    uint8\_t x;

    uint16\_t crc = 0xFFFF;

    while (length--) {

        x = crc >> 8 ^ \*data\_p++;

        x ^= x >> 4;

        crc = (crc << 8) ^ ((uint16\_t)(x << 12)) ^ ((uint16\_t)(x << 5)) ^ ((uint16\_t)x);

    }

    return swap16(crc);

}

### UAT Aircraft Message

#U:ICAO,UAT\_FLAGS,CALL,SQUAWK,ECAT,LAT,LON,BARO\_ALT,GNSS\_ALT,DIR,SPEED,BARO\_VRATE,GNSS\_VRATE,UAT\_EMERG,NICNAC,ACDIMS,VERSION,SIGS,SIGQ,UATFPS,CRC\r\n

|  |  |  |  |
| --- | --- | --- | --- |
| **Field** | **Description** | **Format** | **Example value** |
| #U | UAT aircraft message start indicator. |  |  |
| ICAO | ICAO number of aircraft (3 bytes). | Hex Integer | 3C65AC |
| UAT\_FLAGS | Flags bitfield, see table 4.1.2.1. | Hex Integer | 12F356A8 |
| CALL | Callsign of aircraft. | String | N61ZP |
| SQUAWK | SQUAWK of aircraft. | Octal Integer | 7232 |
| ECAT | Emitter category, see table 4.1.1.2. | Integer | 14 |
| LAT | Latitude, in degrees. | Float | 57.57634 |
| LON | Longitude, in degrees. | Float | 17.59554 |
| BARO\_ALT | Barometric altitude, in feet. | Integer | 5000 |
| GNSS\_ALT | Geometric altitude, in feet. | Integer | 5000 |
| DIR | Direction of aircraft, in degrees [0,360). Consult bit flags to determine whether this field is true heading, magnetic heading, or track. | Integer | 35 |
| SPEED | Horizontal velocity of aircraft, in knots. | Integer | 464 |
| BARO\_VRATE | Barometric vertical velocity of aircraft, in ft/min. | Integer | -1344 |
| GNSS\_VRATE | Geometric vertical velocity of the aircraft, in ft/min | Integer | -1344 |
| UAT\_EMERG | Aircraft UAT emergency / priority status. See table. | Integer | 0 |
| NICNAC | Aircraft data integrity. See table 4.1.1.3 | Hex Integer |  |
| ACDIMS | Aircraft physical dimensions and system design assurance. See table 4.1.1.4. | Hex Integer | 31BE89F2 |
| VERSION | UAT protocol version used by the aircraft. | Integer | 1 |
| SIGS | Signal strength, in dBm. | Integer | -92 |
| SIGQ | Number of bits corrected using UAT forward error correction. 0 (best), 6 (worst). | Integer | 2 |
| UATFPS | Number of valid UAT frames received from the aircraft in the last second. | Integer | 1 |
| CRC | CRC16 (described in 4.1.1.5). | Hex Integer | 2D3E |

NOTE: See Mode S Aircraft message decoding reference for any bitfields not prefixed with “UAT\_”.

#### UAT\_FLAGS Bitfield

|  |  |  |
| --- | --- | --- |
| **Bit** | **Bit Name** | **Meaning if the bit is set (1)** |
| 0 | IS\_AIRBORNE | Emitter is airborne. |
| 1 | BARO\_ALTITUDE\_VALID | Emitter has provided a barometer altitude. |
| 2 | GNSS\_ALTITUDE\_VALID | Emitter has provided a GNSS altitude. |
| 3 | POSITION\_VALID | Emitter has provided a pair of even and odd Compact Position Reporting packets that were decoded to a location. |
| 4 | DIRECTION\_VALID | Emitter has provided a direction (may be ground track, magnetic compass heading, or true compass heading). |
| 5 | HORIZONTAL\_SPEED\_VALID | Emitter has provided a horizontal velocity. |
| 6 | BARO\_VERTICAL\_RATE\_VALID | Emitter has provided a barometric vertical velocity. |
| 7 | GNSS\_VERTICAL\_RATE\_VALID | Emitter has provided a GNSS vertical velocity. |
| 8 | HAS\_CDTI | Aircraft has Cockpit Display of Traffic Information (CDTI) equipped. |
| 9 | TCAS\_OPERATIONAL | Aircraft is equipped with an operational TCAS / ACAS system. |
| 10 | DIRECTION\_IS\_HEADING | Surface position messages provided by the aircraft indicate a heading and not a track angle. |
| 11 | HEADING\_USES\_MAGNETIC\_NORTH | Heading reported by the aircraft while on the surface uses magnetic north instead of true north. |
| 12 | IDENT | The aircraft has its SPI (Special Position Identification) bits set in Mode A/C or Mode S messages. This indicates that the pilot has depressed the momentary IDENT switch on their transponder, most likely at the request of air traffic control. |
| 13-14 Reserved | | |
| 15 | TCAS\_RA | The aircraft has an active TCAS resolution advisory (i.e. the aircraft is warning the pilot to take action in order to avoid colliding with another aircraft). |
| 16 | RECEIVING\_ATC\_SERVICES |  |
| 17-22 Reserved | | |
| 23 | UPDATED\_BARO\_ALTITUDE | Barometric altitude has been updated within the last reporting interval. |
| 24 | UPDATED\_GNSS\_ALTITUDE | GNSS altitude has been updated within the last reporting interval. |
| 25 | UPDATED\_POSITION | Position (latitude / longitude) has been updated within the last reporting interval. |
| 26 | UPDATED\_DIRECTION | Direction has been updated within the last reporting interval. |
| 27 | UPDATED\_HORIZONTAL\_SPEED | Horizontal velocity has been updated within the last reporting interval. |
| 28 | UPDATED\_BARO\_VERTICAL\_RATE | Barometric vertical velocity has been updated within the last reporting interval. |
| 29 | UPDATED\_GNSS\_VERTICAL\_RATE | GNSS vertical velocity has been updated within the last reporting interval. |
| 30-31 Reserved | | |

#### UAT\_EMERG Bitfield

Contains the emergency / priority status reported by a UAT emitter.

|  |  |
| --- | --- |
| **UAT\_EMERG Value** | **Meaning** |
| 0 | No emergency. |
| 1 | General emergency. |
| 2 | Lifeguard / medical emergency. |
| 3 | Minimum fuel. |
| 4 | No communications. |
| 5 | Unlawful interference. |
| 6 | Downed aircraft. |
| 7 | Reserved. |

### Statistics Message

This message contains some useful statistics about ADSBee’s operational status. Format of that frame is shown below:

#S:VERSION,DPS,RAW\_SFPS,SFPS,RAW\_ESFPS,ESFPS,RAW\_UATFPS,UATFPS,TSCAL,UPTIME,CRC\r\n

|  |  |  |  |
| --- | --- | --- | --- |
| **Field** | **Description** | **Format** | **Example Value** |
| #S | Statistics message start indicator. |  |  |
| VERSION | Version of the CSBee protocol being used. | Integer | 2 |
| SDPS | Number of attempted Mode S demodulations in the last second. | Integer | 106 |
| RAW\_SFPS | Number of squitter (56-bit Mode S) frames received in the last second. | Integer | 150 |
| SFPS | Number of valid squitter (56-bit Mode S) frames received in the last second. | Integer | 20 |
| RAW\_ESFPS | Number of extended squitter (112-bit Mode S) frames received in the last second. | Integer | 15 |
| ESFPS | Number of valid Mode S frames received in the last second. | Integer | 3 |
| RAW\_UATFPS | Number of UAT frames received in the last second. | Integer | 5 |
| UATFPS | Number of valid UAT frames received in the last second. | Integer | 4 |
| NUM\_AIRCRAFT | Number of aircraft tracked in the last second. | Integer | 20 |
| TSCAL | Calibration value for TS field in raw frames | Integer | 13999415 |
| UPTIME | Receiver uptime, in seconds. | Integer | 13456 |
| CRC | CRC16 (described in 4.1.3.1). | Hex Integer | 2D3E |

#### CRC Field

See 4.1.1.5.

## GDL90

ADSBee complies with the GDL90 public data interface specification [560-1058-00 Rev A](https://www.faa.gov/sites/faa.gov/files/air_traffic/technology/adsb/archival/GDL90_Public_ICD_RevA.PDF).

## MAVLINK

Tracked aircraft information is sent in MAVLINK ADSB\_VEHICLE messages, in a data burst once per second. The data burst consists of 1x MAVLINK Heartbeat message, Nx ADSB\_VEHICLE messages, where N is the number of tracked aircraft, and 1x special delimiter message (MAVLINK\_REQUEST\_DATA\_STREAM for MAVLINK1 mode, MAVLINK\_MESSAGE\_INTERVAL for MAVLINK2 mode) which indicates the end of the list of tracked aircraft. Note that this is a binary protocol which is not human readable.

|  |
| --- |
| **WARNING**: [Windows has a bug](https://www.guralp.com/howtos/misindentified-serial-mouse.shtml#:~:text=The%20COM%20port%20then%20becomes,cause%20the%20PC%20to%20crash.), which causes some machines to recognize a serial port reporting MAVLINK packets as a mouse, which can result in phantom mouse movements and clicks (ask me how I know). Please use caution while running MAVLINK on a serial port while the computer is unattended. |

### MAVLINK\_HEARTBEAT （Message ID 0） Packet Definition

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Field Name** | **Type** | **Units** | **Values** | **Description** |
| custom\_mode | uint32\_t |  | 0 | Unused. |
| type | uint8\_t |  | MAV\_TYPE\_ADSB | Always MAV\_TYPE\_ADSB (27). |
| autopilot | uint8\_t |  | MAV\_AUTOPILOT\_INVALID | Always MAV\_AUTOPILOT\_INVALID (8). |
| base\_mode | uint8\_t |  | 0 | Unused. |
| system\_status | uint8\_t |  | MAV\_STATE\_ACTIVE | Always MAV\_STATE\_ACTIVE (4). |
| mavlink\_version | uint8\_t |  | MAVLINK\_VERSION | 1 for MAVLINK1 mode, 2 for MAVLINK2 mode. |

### MAVLINK ADSB\_VEHICLE (Message ID 246) Packet Definition

From: [https://mavlink.io/en/messages/common.html#ADSB\_VEHICLE](https://mavlink.io/en/messages/common.html%23ADSB_VEHICLE)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Field Name** | **Type** | **Units** | **Values** | **Description** |
| ICAO\_address | uint32\_t |  |  | ICAO address |
| lat | int32\_t | degE7 |  | Latitude |
| lon | int32\_t | degE7 |  | Longitude |
| altitude\_type | uint8\_t |  | [ADSB\_ALTITUDE\_TYPE](https://mavlink.io/en/messages/common.html#ADSB_ALTITUDE_TYPE) | ADSB altitude type. |
| altitude | int32\_t | mm |  | Altitude(ASL) |
| heading | uint16\_t | cdeg |  | Course over ground |
| hor\_velocity | uint16\_t | cm/s |  | The horizontal velocity |
| ver\_velocity | int16\_t | cm/s |  | The vertical velocity. Positive is up |
| callsign | char[9] |  |  | The callsign, 8+null |
| emitter\_type | uint8\_t |  | [ADSB\_EMITTER\_TYPE](https://mavlink.io/en/messages/common.html#ADSB_EMITTER_TYPE) | ADSB emitter type. |
| tslc | uint8\_t | s |  | Time since last communication in seconds |
| flags | uint16\_t |  | [ADSB\_FLAGS](https://mavlink.io/en/messages/common.html#ADSB_FLAGS) | Bitmap to indicate various statuses including valid data fields |
| squawk | uint16\_t |  |  | Squawk code |

### MAVLINK\_REQUEST\_DATA\_STREAM (Message ID 66) Packet Definition

This message serves as the delimiter which indicates the end of the aircraft list in MAVLINK1 mode.

|  |  |  |  |
| --- | --- | --- | --- |
| **Field Name** | **Type** | **Units** | **Description** |
| req\_message\_rate | uint16\_t |  | Always 0 (unused). |
| target\_system | uint8\_t |  | Always 0 (unused). |
| target\_component | uint8\_t |  | Always 0 (unused). |
| req\_stream\_id | uint8\_t |  | Always 0 (unused). |
| start\_stop | uint8\_t |  | Always 0 (unused). |

### MAVLINK MESSAGE\_INTERVAL (Message ID 244) Packet Definition

This message serves as the delimiter which indicates the end of the aircraft list in MAVLINK2 mode.

From: [https://mavlink.io/en/messages/common.html#MESSAGE\_INTERVAL](https://mavlink.io/en/messages/common.html%23MESSAGE_INTERVAL)

|  |  |  |  |
| --- | --- | --- | --- |
| **Field Name** | **Type** | **Units** | **Description** |
| message\_id | uint16\_t |  | The ID of the requested MAVLink message. v1.0 is limited to 254 messages.  NOTE: For ADSBee 1090, message\_id is always 246, corresponding to the ADSB\_VEHICLE message. |
| interval\_us | int32\_t | us | The interval between two messages. A value of -1 indicates this stream is disabled, 0 indicates it is not available, > 0 indicates the interval at which it is sent.  NOTE: For ADSBee 1090, message\_id is always 1000 us. |

## Mode S Beast

Mode S Beast is a popular feed protocol used by both open-source and commercial data exchanges to send Mode S data, often over TCP sockets or serial connections.

Mode S Beast sends packets as raw binary, with 0x1a used as an “escape” character indicating the start of a Beast frame. Any non start-of-frame instance of 0x1a is escaped with an additional 0x1a beforehand. Thus, 0x1a can be interpreted as the start of a Beast frame, and 0x1a1a can be interpreted as a 0x1a value within a Beast frame.

### Beast: Mode S Frames

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Field** | **Frame Start** | **Frame Type** | **Timestamp** | **RSSI** | **Payload** |
| Length [Bytes] | 1 | 1 | 6-12 | 1-2 | Mode S Short: 7-14  Mode S Long: 14-28 |
| Example | 0x1a | 0x32 | 0x123456781a1aff | 0x56 | <data> |
| Definition | 0x1a  Frame start is always an escape char. | 0x32: Mode S Short  0x33: Mode S Long  No escapes. | 6-byte 12MHz MLAT timestamp, MSB first.  May have up to 6 escapes. | RSSI byte is “Beast Power Level”, which is the square root of the un-logged dBFS value.  May have up to 1 escape. | Packet contents.  May theoretically have up to <packet\_length> escapes, but this would not correspond to a valid packet and will not be seen in practice. |

### Beast: UAT Frames

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Field** | **Frame Start** | **Frame Type** | **UAT Message Type** | **Timestamp** | **RSSI** | **Payload** |
| Length [Bytes] | 1 | 1 | 1 | 6-12 | 1-2 | UAT Short ADSB: |
| Example | 0x1a | 0xec | 0x73 | 0x123456781a1aff | 0x56 | <data> |
| Definition | 0x1a  Frame start is always an escape char. | 0xec  Indicates frame type UAT (both ADSB and uplink).  No escapes. | 0x73 (‘s’): UAT short ADSB (30 byte payload, not including escapes).  0x5c (‘l’): UAT long ADSB (48 byte payload, not including escapes)  0x75 (‘u’): UAT Uplink (552 byte payload, not including escapes)  No escapes. | 6-byte 12MHz MLAT timestamp, MSB first.  May have up to 6 escapes. | RSSI byte is “Beast Power Level”, which is the square root of the un-logged dBFS value.  May have up to 1 escape. | Packet contents, including both payload and FEC parity.  Uplink packets remain interleaved (transmitted byte order retained).  May theoretically have up to <packet\_length> escapes, but this would not correspond to a valid packet and will not be seen in practice. |

## Raw Packets

### Raw Mode S Frames

Raw Mode S packets are reported in the format below. Only packets that have passed checksum validation and match a supported Mode S downlink format are reported.

#MDS\*RAW\_FRAME;(SOURCE,SIGS,SIGQ,TS)\r\n

|  |  |  |  |
| --- | --- | --- | --- |
| **Field** | **Description** | **Format** | **Example value** |
| #MDS | Indicates the start of a raw Mode S frame. |  |  |
| RAW\_FRAME | The packet contents as raw hexadecimal. Varies in length depending on packet length. | Hexadecimal String | 8D48C22D60AB0452BFAD19A695E0 |
| SOURCE | An unsigned integer | int16\_t | 2 |
| SIGS | Signal strength of the packet in dBm, printed as a decimal value. | int16\_t | -60 |
| SIGQ | Signal quality of the packet in dB, printed as a decimal value. | int16\_t | 2 |
| TS | 64-bit 48MHz MLAT counter ticks, printed as a hexadecimal string. | uint64\_t | 00000000FB671342 |

### Raw UAT ADSB Frames

Raw UAT frames are reported in the format below. Only packets that have passed checksum validation are reported. Note that UAT uplink frames can be quite long (552 Bytes / 1104 chars), so serial buffers need to be able to handle this!

#UAT\*-RAW\_FRAME;(SIGS,SIGQ,TS)\r\n

|  |  |  |  |
| --- | --- | --- | --- |
| **Field** | **Description** | **Format** | **Example value** |
| #UAT | Indicates the start of a raw UAT frame. |  |  |
| RAW\_FRAME | The packet contents as raw hexadecimal. Varies in length depending on packet length. | Hexadecimal String |  |
| SIGS | Signal strength of the packet in dBm. | int16\_t | -60 |
| SIGQ | Signal quality of the packet in dB. | int16\_t | 2 |
| TS | 64-bit MLAT counter value in hexadecimal format. | uint64\_t | 00000000FB671342 |

### Raw UAT Uplink Frames

Raw UAT uplink frames are reported in the format below. Only packets that have passed checksum validation are reported. Note that UAT uplink frames can be quite long (552 Bytes / 1104 chars), so serial buffers need to be able to handle this!

#UAT\*+RAW\_FRAME;(SIGS,SIGQ,TS)\r\n

|  |  |  |  |
| --- | --- | --- | --- |
| **Field** | **Description** | **Format** | **Example value** |
| #UAT | Indicates the start of a raw UAT frame. |  |  |
| RAW\_FRAME | The packet contents as raw hexadecimal. Varies in length depending on packet length. | Hexadecimal String |  |
| SIGS | Signal strength of the packet in dBm. | int16\_t | -60 |
| SIGQ | Signal quality of the packet in dB. | int16\_t | 2 |
| TS | 64-bit MLAT counter value in hexadecimal format. | uint64\_t | 00000000FB671342 |